;; Realtek 10/100/1000 PCI-E NIC Family all in one NDIS Driver
;;
;; Copyright 2008, Realtek Semiconductor Corporation
;;
;; .this release is primarily for motherboard OEM for WHQL test.

[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %Realtek%                               
CatalogFile.NT = netrtle.cat                        ;;for WHQL certified
DriverVer      = 01/03/2008,5.686.0103.2008

[Manufacturer]
%Realtek%      = Realtek, NTx86.5.1, NTamd64

[ControlFlags]
ExcludeFromSelect = *

[Realtek]
; DisplayName            Section            DeviceID
; -----------            -------            --------
;8101E
%RTL8136.DeviceDesc%    = RTL8136.ndi,      PCI\VEN_10EC&DEV_8136&REV_01
%RTL8136.DeviceDesc%    = RTL8136.ndi,      PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_01
;8101HP
%RTL8136.DeviceDesc%    = RTL8136HP.ndi,    PCI\VEN_10EC&DEV_8136&SUBSYS_2A57103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HP.ndi,    PCI\VEN_10EC&DEV_8136&SUBSYS_2A78103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HP.ndi,    PCI\VEN_10EC&DEV_8136&SUBSYS_2A79103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HP.ndi,    PCI\VEN_10EC&DEV_8136&SUBSYS_FF101179&REV_01 ;Toshiba

;8102E
%RTL8102.DeviceDesc%    = RTL8102.ndi,      PCI\VEN_10EC&DEV_8136&REV_02
%RTL8102.DeviceDesc%    = RTL8102.ndi,      PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_02
%RTL8102.DeviceDesc%    = RTL8102.ndi,      PCI\VEN_10EC&DEV_8136&SUBSYS_30F2103C ;HP
%RTL8102.DeviceDesc%    = RTL8102.ndi,      PCI\VEN_10EC&DEV_8136&SUBSYS_3602103C ;HP
%RTL8102.DeviceDesc%    = RTL8102.ndi,      PCI\VEN_10EC&DEV_8136&SUBSYS_3603103C ;HP

;8168B
%RTL8168.DeviceDesc%    = RTL8168.ndi,      PCI\VEN_10EC&DEV_8168&REV_01
%RTL8168.DeviceDesc%    = RTL8168.ndi,      PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_01
;8168C
%RTL8168C.DeviceDesc%   = RTL8168C.ndi,     PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%   = RTL8168C.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02
;8168CASUS
%RTL8168C.DeviceDesc%   = RTL8168CASUS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82FF1043&REV_02 ;ASUS

[Realtek.NTx86.5.1]; This section will only be installed by Windows XP
;8101E
%RTL8136.DeviceDesc%	= RTL8136x.ndi,	    PCI\VEN_10EC&DEV_8136&REV_01
%RTL8136.DeviceDesc%	= RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_01
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_108D147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_180E147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C3C147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_240F147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_010C1025&REV_01 ;acer
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0618A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_063DA0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0631A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0634A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0636A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0640A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2055161F&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_206A161F&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_206B161F&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0560107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0561107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0565107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0566107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_12F51043&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_12F61043&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C10A1631&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2101631&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2121631&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_53498086&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_D6068086&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0001940&REV_01 ;Channel
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_027D1028&REV_01 ;DELL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_027E1028&REV_01 ;DELL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0F821019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0F961019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_81361019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90A21019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90AE1019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_906B1019&REV_01 ;ECS(intel)
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90AC1019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B11019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90371695&REV_01 ;Epox
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_601F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60251509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60291509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60401509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60411509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60421509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60431509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60441509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60451509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60461509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60471509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60481509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60491509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604A1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604B1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604C1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604D1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604E1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0C40105B&REV_01 ;Fox
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0C76105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0CE6105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D1B105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D1C105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D40105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D41105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D42105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D43105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D44105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D48105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D4A105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DE2105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DE3105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DF2105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11231734&REV_01 ;FSC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11361734&REV_01 ;FSC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11371734&REV_01 ;FSC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_113A1734&REV_01 ;FSC(P1)
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0380107B&REV_01 ;GATEWAY
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0381107B&REV_01 ;GATEWAY
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0386107B&REV_01 ;GATEWAY
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0001458&REV_01 ;Gigabyte
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_301A17AA&REV_01 ;Gigabyte
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10128086&REV_01 ;INTEL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_D6078086&REV_01 ;INTEL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00161170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00371170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00411170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813616F3&REV_01 ;JETWAY
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_302917AA&REV_01 ;Lenovo
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_303017AA&REV_01 ;Lenovo
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01151854&REV_01 ;LGE
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01161854&REV_01 ;LGE
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_82521071&REV_01 ;MiTAC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_276C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_302C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_313C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_314C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_327C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_337C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_367C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_368C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_369C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_373C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_376C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_379C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_382C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_387C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FB71462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FE91462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FF31462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_44101462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_501C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_525C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_528C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_63F11462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_63F61462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_66101462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_732A1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_732B1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10271631&REV_01 ;NEC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C0271631&REV_01 ;NEC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C10C1631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0311631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0368107B&REV_01 ;RT-QTA
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_104D13BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105013BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105213BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105313BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105413BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF001179&REV_01 ;Toshiba(Compal)
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF011179&REV_01 ;Toshiba(Compal)
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF311179&REV_01 ;Toshiba
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF501179&REV_01 ;Toshiba
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1091147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C41147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C43147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C46147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2B301584&REV_01 ;Uniwill
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_97001584&REV_01 ;Uniwill
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_A01414FF&REV_01 ;WHITE BOX
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105317C0&REV_01 ;Wistron


;8101HP
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A57103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A78103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A79103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_FF101179&REV_01 ;Toshiba

;8102E
%RTL8102.DeviceDesc%	= RTL8102x.ndi,	    PCI\VEN_10EC&DEV_8136&REV_02
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_02
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02741028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90AE1019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B31019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B41019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11361734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11371734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30DE103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30F2103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30FB103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30FE103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3600103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3602103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3603103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17721854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17731854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2141631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2151631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2161631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2171631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2181631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2191631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0772152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0773152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF1C1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF1E1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF601179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF621179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF641179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF661179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF681179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF6A1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003014C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003114C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003214C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003314C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003414C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003514C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003614C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003714C0&REV_02 ;WB


;8168B
%RTL8168.DeviceDesc%	= RTL8168x.ndi,	    PCI\VEN_10EC&DEV_8168&REV_01
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_01
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1071147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1072147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1073147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1074147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1077147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1078147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1079147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_107A147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_108D147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C3C147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_240D147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2410147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2412147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01071025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_010C1025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01261025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E0B105B&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B1331897&REV_01 ;AMTEK
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B2201897&REV_01 ;AMTEK
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_060DA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0611A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0614A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0616A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_061BA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_061CA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0623A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0624A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0625A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_063EA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0642A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2055161F&REV_01 ;Arima
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_206A161F&REV_01 ;Arima
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_206B161F&REV_01 ;Arima
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_11F51043&REV_01 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_81AA1043&REV_01 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0001940&REV_01 ;Channel
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05211558&REV_01 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05911558&REV_01 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_09021558&REV_01 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_002014C0&REV_01 ;Compal
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_002114C0&REV_01 ;Compal
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_88071033&REV_01 ;Compal
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_02591028&REV_01 ;DELL
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_02781028&REV_01 ;DELL
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F711019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F721019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F761019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F771019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F811019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F821019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_81681019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_902A1019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0151631&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_90361695&REV_01 ;Epox
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_601F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60251509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60291509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801A1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801C1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801D1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801E1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C40105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C76105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7D105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7E105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C88105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C89105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C90105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C91105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C92105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0CE6105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0CE7105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D0B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D0E105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D1B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D1C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D40105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D41105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D42105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D48105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DF9105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D43105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D44105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DE2105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DE3105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DF2105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E0F105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E11105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_111C1734&REV_01 ;FSC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113B1734&REV_01 ;FSC(P15)
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113D1734&REV_01 ;FSC(X17)
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113E1734&REV_01 ;FSC(S13)
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_01 ;FSC(D45/D46)
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0690107B&REV_01 ;GATEWAY
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_01 ;Gigabyte
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_30B6103C&REV_01 ;HP Notebook
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_30CC103C&REV_01 ;HP Notebook
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_D6088086&REV_01 ;INTEL
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_00401170&REV_01 ;Inventec
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_500E17FF&REV_01 ;Inventec
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816816F3&REV_01 ;JETWAY
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_302917AA&REV_01 ;Lenovo
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_303017AA&REV_01 ;Lenovo
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01171854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01181854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01191854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_011A1854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_47001071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_47011071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_82521071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B3001071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03411462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03711462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05311462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05711462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_238C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_270C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_276C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_279C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_280C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2F811462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FB11462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FB31462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FBD1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_302C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_309C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_327C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33201462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33371462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33411462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_334B1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_337C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_338C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33FF1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_34131462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_345C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_348C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_356C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_367C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_368C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_373C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_375C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_376C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_379C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_384C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_387C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3F711462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FB71462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FB91462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FCC1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FD51462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FDF1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FE91462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FF31462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FF41462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FFE1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42CD1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42D71462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42E11462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43101462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43141462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43241462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43271462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_514C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63701462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63F21462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63F41462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_65101462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_72101462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_73271462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_732A1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_732B1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80111854&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80161854&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80171854&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A4121462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A4221462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E9011631&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E9021631&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_18548011&REV_01 ;MSI_SI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_88071033&REV_01 ;NEC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0151631&REV_01 ;NEC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_887E1033&REV_01 ;NEC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_058F17FF&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0761152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0762152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0763152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_104D13BD&REV_01 ;Sharp
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_105013BD&REV_01 ;Sharp
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_FF001179&REV_01 ;Toshiba(Compal)
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_FF011179&REV_01 ;Toshiba(Compal)
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1091147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C41147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C43147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C46147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_10CD1734&REV_01 ;Uniwill(FSC)
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_90761584&REV_01 ;Uniwill
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_110E1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_105317C0&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_10C317C0&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A00D14FF&REV_01 ;XPLORE

;8168C
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_13601019&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_063AA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0643A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0644A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0646A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_16D51043&REV_02 ;ASUS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_C2111631&REV_02 ;ASUS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_C2131631&REV_02 ;ASUS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080017FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080117FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_302C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_313C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_398C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_501C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_513C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_519C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_528C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_03901558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04811558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_072F1558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_08051558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_08061558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_08601558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_70011558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_76401558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_76411558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02581028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02591028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02781028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02791028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_027D1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_027E1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02821028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02831028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02851028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_81111019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_81681019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90AD1019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90AE1019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60411509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60421509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60431509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60441509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60451509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60461509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60471509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60481509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60491509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604A1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604B1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604C1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604D1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604E1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604F1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_802C1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D0B105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D48105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DE3105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DF0105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E0F105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E11105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_11351734&REV_02 ;FSC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113B1734&REV_02 ;FSC(P15)
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113D1734&REV_02 ;FSC(X17)
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113E1734&REV_02 ;FSC(S13)
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_02 ;FSC(D45/D46)
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A6F103C&REV_02 ;HP cPC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A73103C&REV_02 ;HP bPC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A74103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3038103C ;HP-CDC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_303A103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_303B103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30DE103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F1103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F2103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F4103C ;HPQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F8103C ;HPQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30FC103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3600103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3602103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3603103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_D6098086&REV_02 ;INTEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01171854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01181854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01191854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_011A1854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_011F1854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01201854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01211854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01221854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17721854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17731854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_392C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_515C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_520C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_536C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_63F51462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_65201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_67101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_67201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_72201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75331462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0772152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0773152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_82E919DB&REV_02 ;TCL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_210817AA&REV_02 ;THINKPAD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1C1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1E1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF601179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF621179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003014C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003114C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003214C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003314C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003414C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003514C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003614C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003714C0&REV_02 ;WB


;8168CASUS
%RTL8168C.DeviceDesc%   = RTL8168CASUSx.ndi,PCI\VEN_10EC&DEV_8168&SUBSYS_82FF1043&REV_02 ;ASUS

[Realtek.NTamd64]; This section will only be installed by Windows XP 64-bit
;8101E
%RTL8136.DeviceDesc%	= RTL8136a.ndi,	    PCI\VEN_10EC&DEV_8136&REV_01
%RTL8136.DeviceDesc%	= RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_01
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_108D147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_180E147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C3C147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_240F147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_010C1025&REV_01 ;acer
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0618A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_063DA0A0&REV_01 ;AOPEN
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2055161F&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_206A161F&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_206B161F&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0560107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0561107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0565107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0566107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_12F51043&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_12F61043&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C10A1631&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2101631&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2121631&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0001940&REV_01 ;Channel
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_027D1028&REV_01 ;DELL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_027E1028&REV_01 ;DELL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0F821019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0F961019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_81361019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_902A1019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_906B1019&REV_01 ;ECS(INTEL)
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90AC1019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90AE1019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B11019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90371695&REV_01 ;Epox
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_601F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60251509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60291509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60401509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60411509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60421509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60431509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60441509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60451509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60461509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60471509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60481509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60491509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604A1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604B1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604C1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604D1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604E1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0C40105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0C76105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0CE6105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D1B105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D1C105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D40105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D41105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D42105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D43105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D44105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D48105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D4A105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DE2105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DE3105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DF2105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11231734&REV_01 ;FSC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11361734&REV_01 ;FSC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11371734&REV_01 ;FSC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_113A1734&REV_01 ;FSC(P1)
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0380107B&REV_01 ;GATEWAY
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0381107B&REV_01 ;GATEWAY
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0386107B&REV_01 ;GATEWAY
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0001458&REV_01 ;GBT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_301A17AA&REV_01 ;GIGABYTE
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10128086&REV_01 ;INTEL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_D6078086&REV_01 ;INTEL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00161170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00371170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00411170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813616F3&REV_01 ;JETWAY
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_302917AA&REV_01 ;Lenovo
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_303017AA&REV_01 ;Lenovo
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01151854&REV_01 ;LGE
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01161854&REV_01 ;LGE
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_82521071&REV_01 ;MiTAC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_276C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_302C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_313C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_314C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_327C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_337C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_367C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_368C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_373C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_376C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_382C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_387C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_379C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FB71462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FE91462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FF31462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_44101462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_501C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_525C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_528C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_63F11462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_63F61462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_66101462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_501C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_732A1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_732B1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10271631&REV_01 ;NEC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C0271631&REV_01 ;NEC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C10C1631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0311631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0368107B&REV_01 ;RT-QTA
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_104D13BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105013BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105213BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105313BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105413BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF001179&REV_01 ;Toshiba(Compal)
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF011179&REV_01 ;Toshiba(Compal)
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF311179&REV_01 ;Toshiba
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF501179&REV_01 ;Toshiba
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1091147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C41147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C43147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C46147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2B301584&REV_01 ;Uniwill
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_97001584&REV_01 ;Uniwill
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_A01414FF&REV_01 ;WHITEBOX
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105317C0&REV_01 ;Wistron
;8101HP
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A57103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A78103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A79103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_30CB103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_FF101179&REV_01 ;Toshiba

;8102E
%RTL8102.DeviceDesc%	= RTL8102a.ndi,	    PCI\VEN_10EC&DEV_8136&REV_02
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_02
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02741028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90AE1019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B31019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B41019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11361734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11371734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30DE103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30F2103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30FB103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30FE103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3600103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3602103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3603103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17721854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17731854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2141631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2151631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2161631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2171631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2181631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2191631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0772152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0773152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF1C1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF1E1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF601179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF621179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF641179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF661179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF681179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF6A1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003014C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003114C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003214C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003314C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003414C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003514C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003614C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003714C0&REV_02 ;WB


;8168B
%RTL8168.DeviceDesc%  	= RTL8168a.ndi,	    PCI\VEN_10EC&DEV_8168&REV_01
%RTL8168.DeviceDesc%	= RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_01
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1077147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1078147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1079147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_107A147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_108D147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C3C147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_240D147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2410147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2412147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01071025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_010C1025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01261025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E0B105B&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B1331897&REV_01 ;AMTEK
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B2201897&REV_01 ;AMTEK
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_060DA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0611A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0614A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0616A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_061BA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_061CA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0623A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0624A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0625A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0631A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0634A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_063EA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0636A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0640A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0642A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2055161F&REV_01 ;Arima
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_206A161F&REV_01 ;Arima
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_206B161F&REV_01 ;Arima
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_11F51043&REV_01 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_81AA1043&REV_01 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_53498086&REV_01 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_D6068086&REV_01 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0001940&REV_01 ;Channel
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05211558&REV_01 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05911558&REV_01 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_09021558&REV_01 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_002014C0&REV_01 ;Compal
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_002114C0&REV_01 ;Compal
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_88071033&REV_01 ;Compal
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_02591028&REV_01 ;DELL
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_02781028&REV_01 ;DELL
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F711019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F721019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F761019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F771019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F811019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F821019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_81681019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_902A1019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_90361695&REV_01 ;Epox
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_601F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60251509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60291509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801A1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801C1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801D1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801E1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C40105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C76105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7D105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7E105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C88105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C89105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C90105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C91105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C92105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0CE6105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0CE7105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D0B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D0E105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D1B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D1C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D40105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D41105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D42105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D43105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D44105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D48105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DE2105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DE3105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DF2105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DF9105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E0F105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E11105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_111C1734&REV_01 ;FSC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113B1734&REV_01 ;FSC(P15)
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113D1734&REV_01 ;FSC(X17)
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113E1734&REV_01 ;FSC(S13)
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_01 ;FSC(D45/D46)
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0690107B&REV_01 ;GATEWAY
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_01 ;GBT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_30B6103C&REV_01 ;HP Notebook
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_30CC103C&REV_01 ;HP Notebook
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_D6088086&REV_01 ;INTEL
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_00401170&REV_01 ;Inventec
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_500E17FF&REV_01 ;Inventec
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816816F3&REV_01 ;JETWAY
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_302917AA&REV_01 ;Lenovo
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_303017AA&REV_01 ;Lenovo
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01171854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01181854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01191854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_011A1854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_47001071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_47011071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_82521071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B3001071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03411462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03711462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05311462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05711462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_238C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_270C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_276C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_279C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_280C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2F811462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FB11462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FB31462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FBD1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_302C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_309C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_327C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33201462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33371462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33411462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_334B1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_337C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_338C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33FF1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_34131462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_345C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_348C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_356C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_367C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_368C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_369C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_373C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_375C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_376C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_379C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_384C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_387C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3F711462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FB71462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FB91462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FCC1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FD51462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FDF1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FE91462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FF31462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FF41462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FFE1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42CD1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42D71462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42E11462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43101462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43141462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43241462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43271462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_514C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63701462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63F21462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63F41462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_65101462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_72101462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_73271462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_732A1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_732B1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80111854&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80161854&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80171854&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A4121462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A4221462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E9011631&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E9021631&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_18548011&REV_01 ;MSI_SI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_88071033&REV_01 ;NEC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0151631&REV_01 ;NEC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_887E1033&REV_01 ;NEC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_058F17FF&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0761152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0762152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0763152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_104D13BD&REV_01 ;Sharp
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_105013BD&REV_01 ;Sharp
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_FF001179&REV_01 ;Toshiba(Compal)
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_FF011179&REV_01 ;Toshiba(Compal)
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1091147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C41147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C43147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C46147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_10CD1734&REV_01 ;Uniwill(FSC)
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_110E1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_105317C0&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_10C317C0&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A00D14FF&REV_01 ;XPLORE

;8168C
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_13601019&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_063AA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0643A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0644A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0646A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_16D51043&REV_02 ;ASUS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_C2111631&REV_02 ;ASUS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_C2131631&REV_02 ;ASUS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080017FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080117FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_302C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_313C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_398C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_501C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_513C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_519C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_528C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_03901558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04811558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_072F1558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_08051558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_08061558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_08601558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_70011558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_76401558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_76411558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02581028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02591028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02781028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02791028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_027D1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_027E1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02821028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02831028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02851028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_81111019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_81681019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90AD1019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90AE1019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60411509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60421509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60431509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60441509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60451509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60461509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60471509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60481509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60491509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604A1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604B1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604C1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604D1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604E1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604F1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_802C1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D0B105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D48105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DE3105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DF0105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E0F105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E11105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_11351734&REV_02 ;FSC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113B1734&REV_02 ;FSC(P15)
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113D1734&REV_02 ;FSC(X17)
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113E1734&REV_02 ;FSC(S13)
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_02 ;FSC(D45/D46)
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A6F103C&REV_02 ;HP cPC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A73103C&REV_02 ;HP bPC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A74103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3038103C ;HP-CDC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_303A103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_303B103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30DE103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F1103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F2103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F4103C ;HPQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F8103C ;HPQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30FC103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3600103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3602103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3603103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_D6098086&REV_02 ;INTEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01171854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01181854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01191854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_011A1854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_011F1854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01201854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01211854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01221854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17721854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17731854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_392C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_515C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_520C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_536C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_63F51462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_65201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_67101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_67201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_72201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75331462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0772152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0773152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_82E919DB&REV_02 ;TCL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_210817AA&REV_02 ;THINKPAD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1C1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1E1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF601179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF621179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003014C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003114C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003214C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003314C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003414C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003514C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003614C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003714C0&REV_02 ;WB

;8168CASUS
%RTL8168C.DeviceDesc%   = RTL8168CASUSa.ndi,PCI\VEN_10EC&DEV_8168&SUBSYS_82FF1043&REV_02 ;ASUS

;;****************************************************************************
;; Windows 98/ME
;;****************************************************************************
;;RTL8168(98/ME)
[RTL8168.ndi]
DriverVer       = 01/03/2008,686
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68BJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8168C(98/ME)
[RTL8168C.ndi]
DriverVer       = 01/03/2008,686
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8168C ASUS(98/ME)
[RTL8168CASUS.ndi]
DriverVer       = 01/03/2008,686
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = WolCap.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8136(98/ME)
[RTL8136.ndi]
DriverVer       = 01/03/2008,686
AddReg          = rtl8136.id.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8136 HP(98/ME)
[RTL8136HP.ndi]
DriverVer       = 01/03/2008,686
AddReg          = rtl8136.id.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = AutoCrossoverDet.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8102E(98/ME)
[RTL8102.ndi]
DriverVer       = 01/03/2008,686
AddReg          = rtl8136.id.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg
CopyFiles       = Rtlnic.CopyFiles9x

[Rtlnic.CopyFiles9x]
Rtenic.sys,,,2

;;****************************************************************************
;; Windows 2000
;;****************************************************************************
;;RTL8168(W2K)
[RTL8168.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68BJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8168.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8168C(W2K)
[RTL8168C.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8168C.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8168 ASUS(W2K)
[RTL8168CASUS.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8168CASUS.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8136(W2K)
[RTL8136.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8136.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8136 HP(W2K)
[RTL8136HP.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, AutoCrossoverDet.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8136HP.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8102E(W2K)
[RTL8102.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8102.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

[Rtlnic.CopyFiles]
Rtenic.sys,,,2

;;****************************************************************************
;; Windows XP
;;****************************************************************************
;;RTL8168(XP)
[RTL8168x.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68BJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8168x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168C(XP)
[RTL8168Cx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8168Cx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168C ASUS(XP)
[RTL8168CASUSx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8168CASUSx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8136(XP)
[RTL8136x.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8136x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8136HP(XP)
[RTL8136HPx.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, AutoCrossoverDet.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8136HPx.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8102E(XP)
[RTL8102x.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8102x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

[Rtlnic.CopyFilesXP]
Rtenicxp.sys,,,2

;;****************************************************************************
;; Windows XP 64-bit
;;****************************************************************************
;;RTL8168(XP64)
[RTL8168a.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68BJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8168a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168C(XP64)
[RTL8168Ca.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8168Ca.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168C ASUS(XP64)
[RTL8168CASUSa.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8168CASUSa.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8136(XP64)
[RTL8136a.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8136a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8136 HP(XP64)
[RTL8136HPa.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, AutoCrossoverDet.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8136HPa.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog


;;****************************************************************************
;;RTL8102E(XP64)
[RTL8102a.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8102a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

[Rtlnic.CopyFilesX64]
Rtenic64.sys,,,2

;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[rtl8168.id.reg]
HKR,,               MediaType,        0, 1
HKR,,               AdapterType,      0, 5
HKR,,               BusType,          0, 5
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "Rtenic.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,NDIS,           LogDriverName,    0, "RTLE8023"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            DeviceID,         0, "PCI\VEN_10EC&DEV_8168"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"  
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

[rtl8136.id.reg]
HKR,,               MediaType,        0, 1
HKR,,               AdapterType,      0, 5
HKR,,               BusType,          0, 5
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "Rtenic.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,NDIS,           LogDriverName,    0, "RTLE8023"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            DeviceID,         0, "PCI\VEN_10EC&DEV_8136"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"  
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

;;****************************************************************************
;; Del parameters
;;****************************************************************************
[GigPreParams.DelReg]
HKR,Ndi\Params\WakeUpFrame
HKR,,WakeUpFrame
HKR,Ndi\Params\NumTxDesc
HKR,,NumTxDesc
HKR,Ndi\Params\NumRxDesc
HKR,,NumRxDesc
HKR,Ndi\Params\NumTxDescHPQ
HKR,,NumTxDescHPQ
HKR,Ndi\Params\RegVlanid
HKR,,RegVlanid
HKR,Ndi\Params\WakeOnLanSpeed
HKR,,WakeOnLanSpeed
;HKR,Ndi\Params\S5WakeOnLan
;HKR,,S5WakeOnLan
HKR,,SuperSwitch

[TsPreParams.DelReg]
HKR,Ndi\Params\WakeUpFrame
HKR,,WakeUpFrame
HKR,Ndi\Params\NumTxDesc
HKR,,NumTxDesc
HKR,Ndi\Params\NumRxDesc
HKR,,NumRxDesc
HKR,Ndi\Params\NumTxDescHPQ
HKR,,NumTxDescHPQ
HKR,Ndi\Params\RegVlanid
HKR,,RegVlanid
HKR,Ndi\Params\WakeOnLanSpeed
HKR,,WakeOnLanSpeed
;HKR,Ndi\Params\S5WakeOnLan
;HKR,,S5WakeOnLan

;;****************************************************************************
;; common parameters
;;****************************************************************************

[NetworkAddress.reg]
HKR,Ndi\params\NetworkAddress,	ParamDesc,	0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,	type,		0, "edit"
HKR,Ndi\params\NetworkAddress,	default,	0, "000000000000"
HKR,Ndi\params\NetworkAddress,	LimitText,	0, "12"
HKR,Ndi\params\NetworkAddress,	UpperCase,	0, "1"
HKR,Ndi\params\NetworkAddress,	Optional,	0, "1"

[Speed.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR, Ndi\params\DuplexMode\enum,  6,          0, %sd1000full%
HKR,,DuplexMode,0,"1"

[Speed10_100.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR,,DuplexMode,0,"1"

;[TxDescNumber.reg]
;HKR,Ndi\Params\NumTxDesc,         ParamDesc,  0, %TxDescNumber%
;HKR,Ndi\Params\NumTxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumTxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumTxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumTxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumTxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumTxDesc,         Base,       0, "10"
;HKR,,NumTxDesc,0,"256"

;[RxDescNumber.reg]
;HKR,Ndi\Params\NumRxDesc,         ParamDesc,  0, %RxDescNumber%
;HKR,Ndi\Params\NumRxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumRxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumRxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumRxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumRxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumRxDesc,         Base,       0, "10"
;HKR,,NumRxDesc,0,"256"

[68BJumboframe.reg]
HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, %Disabled%
HKR,Ndi\params\Jumboframe\enum,   "1",        0, %2KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "2",        0, %3KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "3",        0, %4KBMTU%
HKR,,Jumboframe,0,"0"

[68CJumboframe.reg]
HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, %Disabled%
HKR,Ndi\params\Jumboframe\enum,   "1",        0, %2KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "2",        0, %3KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "3",        0, %4KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "4",        0, %5KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "5",        0, %6KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "6",        0, %7KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "7",        0, %8KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "8",        0, %9KBMTU%
HKR,,Jumboframe,0,"0"

[Flowctrl.reg]
HKR,Ndi\params\FlowControl,      ParamDesc,  0, %FlowControl%
HKR,Ndi\params\FlowControl,      default,    0, "1"
HKR,Ndi\params\FlowControl,      type,       0, "enum"
HKR,Ndi\params\FlowControl\enum, "0",        0, %Disabled%
HKR,Ndi\params\FlowControl\enum, "1",        0, %Enabled%
HKR,,FlowControl,0,"1" 

[S5Wol.reg]
HKR,Ndi\params\S5WakeOnLan,      ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,      default,    0, "1"
HKR,Ndi\params\S5WakeOnLan,      type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum, "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum, "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"1"

[WolShutdownLinkSpeed.reg]
HKR, Ndi\params\WolShutdownLinkSpeed,       ParamDesc,  0, %WolShutdownLinkSpeed%
HKR, Ndi\params\WolShutdownLinkSpeed,       type,       0, "enum"
HKR, Ndi\params\WolShutdownLinkSpeed,       default,    0, "1"
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "0",        0, %10MbFirst%
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "1",        0, %100MbFirst%
HKR,,WolShutdownLinkSpeed,0,"1"

[WolShutdownLinkSpeedIntel.reg]
HKR, Ndi\params\WolShutdownLinkSpeed,       ParamDesc,  0, %WolShutdownLinkSpeed%
HKR, Ndi\params\WolShutdownLinkSpeed,       type,       0, "enum"
HKR, Ndi\params\WolShutdownLinkSpeed,       default,    0, "2"
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "0",        0, %10MbFirst%
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "1",        0, %100MbFirst%
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "2",        0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"2"

[WolCap.reg]
HKR, Ndi\params\WolCap,            ParamDesc,  0, %WolCap%
HKR, Ndi\params\WolCap,            type,       0, "enum"
HKR, Ndi\params\WolCap,            default,    0, "3"
HKR, Ndi\params\WolCap\enum,       "0",        0, %None%
HKR, Ndi\params\WolCap\enum,       "1",        0, %PatternMatch%
HKR, Ndi\params\WolCap\enum,       "2",        0, %MagicPacket%
HKR, Ndi\params\WolCap\enum,       "3",        0, %PatternAndMagic%
HKR,,WolCap,0,"3"

;[AutoSpeedDown.reg]
;HKR,Ndi\params\AutoSpeedDown,         ParamDesc,  0, %AutoSpeedDown%
;HKR,Ndi\params\AutoSpeedDown,         default,    0, "1"
;HKR,Ndi\params\AutoSpeedDown,         type,       0, "enum"
;HKR,Ndi\params\AutoSpeedDown\enum,    "0",        0, %Disabled%
;HKR,Ndi\params\AutoSpeedDown\enum,    "1",        0, %Enabled%
;HKR,,AutoSpeedDown,0,"1"

;[SuperSwitch.reg]
;HKR,,SuperSwitch,0,"0"

;;****************************************************************************
;; NT parameters
;;****************************************************************************

[OffloadChksum.reg]
HKR,Ndi\params\CksOffload,        ParamDesc,  0, %ChecksumOffload%
HKR,Ndi\params\CksOffload,        default,    0, "1"
HKR,Ndi\params\CksOffload,        type,       0, "enum"
HKR,Ndi\params\CksOffload\enum,   "0",        0, %Disabled%
HKR,Ndi\params\CksOffload\enum,   "1",        0, %TxRxChecksumEnabled%
HKR,Ndi\params\CksOffload\enum,   "3",        0, %RxChecksumEnabled%
HKR,Ndi\params\CksOffload\enum,   "4",        0, %TxChecksumEnabled%
HKR,,CksOffload,0,"1" 

[OffloadLargesend.reg]
HKR,Ndi\params\Largesend,         ParamDesc,  0, %LargesendOffload%
HKR,Ndi\params\Largesend,         default,    0, "1"
HKR,Ndi\params\Largesend,         type,       0, "enum"
HKR,Ndi\params\Largesend\enum,    "0",        0, %Disabled%
HKR,Ndi\params\Largesend\enum,    "1",        0, %Enabled%
HKR,,Largesend,0,"1" 

[VLanTagging.reg]
HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, %Disabled%
HKR,Ndi\params\Support8021p\enum, "1",        0, %Enabled%
HKR,,Support8021p,0,"0" 

;[VLanID.reg]
;HKR,Ndi\Params\RegVlanid,   ParamDesc,  0, %VLanID%
;HKR,Ndi\Params\RegVlanid,   Type,       0, "int"
;HKR,Ndi\Params\RegVlanid,   Default,    0, "0"
;HKR,Ndi\Params\RegVlanid,   Min,        0, "0"
;HKR,Ndi\Params\RegVlanid,   Max,        0, "4094"
;HKR,Ndi\Params\RegVlanid,   Step,       0, "1"
;HKR,Ndi\Params\RegVlanid,   Base,       0, "10"
;HKR,,RegVlanid,0,"0" 

;[TxHPQDescNumber.reg]
;HKR,Ndi\Params\NumTxDescHPQ,      ParamDesc,  0, %TxHPQDescNumber%
;HKR,Ndi\Params\NumTxDescHPQ,      Type,       0, "int"
;HKR,Ndi\Params\NumTxDescHPQ,      Default,    0, "256"
;HKR,Ndi\Params\NumTxDescHPQ,      Min,        0, "64"
;HKR,Ndi\Params\NumTxDescHPQ,      Max,        0, "512"
;HKR,Ndi\Params\NumTxDescHPQ,      Step,       0, "1"
;HKR,Ndi\Params\NumTxDescHPQ,      Base,       0, "10"
;HKR,,NumTxDescHPQ,0,"256" 

[AutoCrossoverDet.reg]
HKR,Ndi\params\AutoCrossoverDet,	ParamDesc,  0, %AutoCrossoverDet%
HKR,Ndi\params\AutoCrossoverDet,	default,    0, "0"
HKR,Ndi\params\AutoCrossoverDet,	type,       0, "enum"
HKR,Ndi\params\AutoCrossoverDet\enum,   "0",        0, %Disabled%
HKR,Ndi\params\AutoCrossoverDet\enum,   "1",        0, %Enabled%
HKR,,AutoCrossoverDet,0,"0"

;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTLE8023.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTLE8023"

[rtsnt.Service]
DisplayName     = %Rtlnic.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtenic.sys
LoadOrderGroup  = NDIS

[RTLE8023xp.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTLE8023xp"

[rtsntxp.Service]
DisplayName     = %Rtlnicxp.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtenicxp.sys
LoadOrderGroup  = NDIS

[RTLE8023x64.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTLE8023x64"

[rtsntx64.Service]
DisplayName     = %Rtlnicx64.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtenic64.sys
LoadOrderGroup  = NDIS

[common.EventLog]
Addreg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
Rtlnic.CopyFiles           = 12
Rtlnic.CopyFilesXP         = 12
Rtlnic.CopyFilesX64        = 12
Rtlnic.CopyFiles9x         = 11
DefaultDestDir             = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
Rtenic.sys	= 1
Rtenicxp.sys	= 1
Rtenic64.sys	= 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p VLAN Tagging"
;VLanID			= "802.1Q VLAN ID"
ChecksumOffload		= "Offload Checksum"
LargesendOffload	= "Offload TCP_LargeSend"
SpeedDuplexMode		= "Link Speed/Duplex Mode"
auto_nego		= "Auto Negotiation"
sd10half		= "10Mbps/Half Duplex"
sd10full		= "10Mbps/Full Duplex"
sd100half		= "100Mbps/Half Duplex"
sd100full		= "100Mbps/Full Duplex"
sd1000full		= "1000Mbps/Full Duplex"
NetworkAddress		= "Network Address"
JumboFrame		= "Jumbo Frame"
;TxDescNumber		= "Number of Tx Descriptor"
;RxDescNumber		= "Number of Rx Descriptor"
;TxHPQDescNumber	= "Number of High Priority Tx Descriptor"
FlowControl		= "Flow Control"
;AutoSpeedDown		= "Auto Speed Down"
S5WakeOnLan		= "Wake-On-Lan After Shutdown"
10MbFirst               = "10 Mbps First"
100MbFirst              = "100 Mbps First"
NotSpeedDown            = "Not Speed Down"
WolShutdownLinkSpeed    = "WOL & Shutdown Link Speed"
AutoCrossoverDet        = "Auto Crossover Detection"
Disabled                = "Disable"
Enabled                 = "Enable"
TxChecksumEnabled       = "Tx Checksum"
RxChecksumEnabled       = "Rx Checksum"
TxRxChecksumEnabled     = "Tx/Rx Checksum"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Wake-On-Lan Capabilities"
None                    = "None"
PatternMatch            = "Pattern Match"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Pattern Match & Magic Packet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek RTL8168/8111 PCI-E Gigabit Ethernet NIC"
RTL8168C.DeviceDesc       = "Realtek RTL8168C(P)/8111C(P) PCI-E Gigabit Ethernet NIC"
RTL8136.DeviceDesc        = "Realtek RTL8139/810x Family Fast Ethernet NIC"
RTL8102.DeviceDesc        = "Realtek RTL8102E Family PCI-E Fast Ethernet NIC" 

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"
